| CustomiOSApi 1.06

- Main Page
- Classes

- Class List
- Class Index
- Class Hierarchy
- Class Members

All Classes Functions Enumerations Enumerator Pages
Instance Methods | List of all members
PrinterStatus Class Reference

This the container class to hold the printer status More...

## Instance Methods
(id) | - initWithStatus:
| Create PrinterStatus object with a value More...
(Boolean) | - IsEqual:
| Compare PrinterStatus object More...
(Boolean) | - StsNOPAPER
(Boolean) | - StsNEARENDPAP
(Boolean) | - StsTICKETOUT
(Boolean) | - StsNOHEAD
(Boolean) | - StsNOCOVER
(Boolean) | - StsSPOOLING
(Boolean) | - StsPAPERROLLING
(Boolean) | - StsLFPRESSED
(Boolean) | - StsFFPRESSED
(Boolean) | - StsOVERTEMP
(Boolean) | - StsHLVOLT
(Boolean) | - StsPAPERJAM
(Boolean) | - StsCUTERROR
(Boolean) | - StsRAMERROR
(Boolean) | - StsEEPROMERROR

## Detailed Description

This the container class to hold the printer status

## Method Documentation

- (id) initWithStatus: |  | (long) | lStatusPrinter |

Create PrinterStatus object with a value

Parameters

  lStatusPrinter | 32bit Status Mask

Returns

- (Boolean) IsEqual: |  | (PrinterStatus *) | printerstatus |

Compare PrinterStatus object

Parameters

  printerstatus | PrinterStatus object

Returns

- (Boolean) StsCUTERROR |  |  |

Indicates that the printer is in CUTTER ERROR Status. Refer to Printer manual to know if this status is supported by the device

- (Boolean) StsEEPROMERROR |  |  |

Indicates that the printer is in EEPROM ERROR Status. Refer to Printer manual to know if this status is supported by the device

- (Boolean) StsFFPRESSED |  |  |

Indicates that the printer is in FFPRESSED Status. Refer to Printer manual to know if this status is supported by the device

- (Boolean) StsHLVOLT |  |  |

Indicates that the printer is in OVERVOLTAGE Status. Refer to Printer manual to know if this status is supported by the device

- (Boolean) StsLFPRESSED |  |  |

Indicates that the printer is in LFPRESSED Status. Refer to Printer manual to know if this status is supported by the device

- (Boolean) StsNEARENDPAP |  |  |

Indicates that the printer is in NEAR PAPER END Status. Refer to Printer manual to know if this status is supported by the device

- (Boolean) StsNOCOVER |  |  |

Indicates that the printer is in COVER OPEN Status. Refer to Printer manual to know if this status is supported by the device

- (Boolean) StsNOHEAD |  |  |

Indicates that the printer is in HEAD UP Status. Refer to Printer manual to know if this status is supported by the device

- (Boolean) StsNOPAPER |  |  |

Indicates that the printer is in NO PAPER Status. Refer to Printer manual to know if this status is supported by the device

- (Boolean) StsOVERTEMP |  |  |

Indicates that the printer is in OVERTEMPERATURE Status. Refer to Printer manual to know if this status is supported by the device

- (Boolean) StsPAPERJAM |  |  |

Indicates that the printer is in PAPER JAM Status. Refer to Printer manual to know if this status is supported by the device

- (Boolean) StsPAPERROLLING |  |  |

Indicates that the printer is in PAPER ROLLING Status. Refer to Printer manual to know if this status is supported by the device

- (Boolean) StsRAMERROR |  |  |

Indicates that the printer is in RAM ERROR Status. Refer to Printer manual to know if this status is supported by the device

- (Boolean) StsSPOOLING |  |  |

Indicates that the printer is in SPOOLING Status. Refer to Printer manual to know if this status is supported by the device

- (Boolean) StsTICKETOUT |  |  |

Indicates that the printer is in TICKET OUT Status. Refer to Printer manual to know if this status is supported by the device