| IDTech Universal SDK 1.0.35.027 API reference for C++

libIDT_VP3300_USB.h
Go to the documentation of this file.
1 #ifndef __LIBIDT_VP3300_USB_H___
2 # define __LIBIDT_VP3300_USB_H___
3
4
5 # define IN
6 # define OUT
7 # define IN_OUT
8 # include "IDTDef.h"
9
15 typedef void (* pMessageHotplug)(int, int);
16
21 typedef void (* pSendDataLog)(BYTE *, int);
22
27 typedef void (* pReadDataLog)(BYTE *, int);
28
33 typedef void (* pEMV_callBack)(int, int, BYTE *, int, IDTTransactionData *, EMV_Callback *, int);
34
39 typedef void (* pMSR_callBack)(int, IDTMSRData);
40
45 typedef void (* pMSR_callBackp)(int, IDTMSRData *);
46
51 typedef void (* pPIN_callBack)(int, IDTPINData *);
52
57 typedef void (* pCMR_callBack)(int, IDTCMRData *);
58
63 typedef void (* pCSFS_callBack)(BYTE status);
64
69 typedef void (* pRKI_callBack)(int,
70 char *);
71
83 typedef void (* ftpComm_callBack)(int, int, int);
84
89 typedef void (* httpComm_callBack)(BYTE *, int);
90
97 typedef void (* v4Comm_callBack)(BYTE, BYTE, BYTE *, int);
98
99
100 # ifdef __cplusplus
101 extern "C" {
102 # endif
103
107 void
108 registerHotplugCallBk(pMessageHotplug pMsgHotplug);
109
113 void
114 registerLogCallBk(pSendDataLog pFSend, pReadDataLog pFRead);
115
120 void
121 device_registerRKICallBk(pRKI_callBack pRKIf);
122
126 void
127 emv_registerCallBk(pEMV_callBack pEMVf);
128
132 void
133 msr_registerCallBk(pMSR_callBack pMSRf);
134
138 void
139 msr_registerCallBkp(pMSR_callBackp pMSRf);
140
144 void
145 ctls_registerCallBk(pMSR_callBack pCTLSf);
146
150 void
151 ctls_registerCallBkp(pMSR_callBackp pCTLSf);
152
156 void
157 pin_registerCallBk(pPIN_callBack pPINf);
158
162 void
163 device_registerCameraCallBk(pCMR_callBack pCMRf);
164
168 void
169 device_registerCardStatusFrontSwitchCallBk(pCSFS_callBack pCSFSf);
170
176 void
177 comm_registerHTTPCallback(httpComm_callBack cBack);
178
184 void
185 comm_registerV4Callback(v4Comm_callBack cBack);
186
191 char *
192 SDK_Version();
193
202 int
203 setAbsoluteLibraryPath(const char * absoluteLibraryPath);
204
212 int
213 device_init();
214
256 int
257 device_setCurrentDevice(int deviceType);
258
265 int
266 device_isAttached(int deviceType);
267
273 int
274 device_close();
275
276
336 void
337 device_getIDGStatusCodeString(IN int returnCode, OUT char * despcrition);
338
339
344 int
345 device_isConnected();
346
357 int
358 device_getFirmwareVersion(OUT char * firmwareVersion);
359
369 int
370 device_getFirmwareVersion_Len(OUT char * firmwareVersion, IN_OUT int * firmwareVersionLen);
371
380 int
381 device_pingDevice();
382
425 int
426 device_controlUserInterface(IN BYTE * values);
427
433 int
434 device_getCurrentDeviceType();
435
436
438 // * Send a Command to device
439 // *
440 // * Sends a command to the device .
441 // *
442 // * @param cmd buffer of command to execute.
443 // * @param cmdLen, the length of the buffer cmd.
444 // *
445 // * @param data buffer of IDG command data.
446 // * @param dataLen, the length of the buffer data.
447 // *
448 // * @param response Response data
449 // * @param respLen, the length of Response data
450 //
451 // * @return RETURN_CODE: Values can be parsed with device_getIDGStatusCodeString()
452 // */
453 //
454 // int device_SendDataCommand(IN BYTE* cmd, IN int cmdLen, IN BYTE* data, IN int dataLen, OUT BYTE* response, IN_OUT int *respLen);
455
472 int
473 device_SendDataCommandNEO(IN int cmd, IN int subCmd, IN BYTE * data, IN int dataLen, OUT BYTE * response,
474 IN_OUT int * respLen);
475
486 int
487 device_enablePassThrough(int enablePassThrough);
488
499 int
500 device_setBurstMode(IN BYTE mode);
501
511 int
512 device_setPollMode(IN BYTE mode);
513
527 int
528 device_setMerchantRecord(int index, int enabled, char * merchantID, char * merchantURL);
529
551 int
552 device_getMerchantRecord(IN int index,
553 OUT BYTE * record);
554
575 int
576 device_getMerchantRecord_Len(IN int index,
577 OUT BYTE * record, IN_OUT int * recordLen);
578
588 int
589 device_getTransactionResults(IDTMSRData * cardData);
590
612 int
613 device_startTransaction(IN double amount, IN double amtOther, IN int type, IN const int _timeout, IN BYTE * tags,
614 IN int tagsLen);
615
620 void
621 device_setTransactionExponent(int exponent);
622
677 int
678 device_activateTransaction(IN const int _timeout, IN BYTE * tags, IN int tagsLen);
679
680
686 int
687 device_cancelTransaction();
688
703 int
704 device_getRTCDateTime(IN BYTE * dateTime, IN_OUT int * dateTimeLen);
705
719 int
720 device_setRTCDateTime(IN BYTE * dateTime, IN int dateTimeLen);
721
731 int
732 device_startRKI(const char * caPath, int isProduction);
733
742 int
743 device_getSDKWaitTime();
744
754 void
755 device_setSDKWaitTime(int waitTime);
756
765 int
766 device_getThreadStackSize();
767
775 void
776 device_setThreadStackSize(int threadSize);
777
788 int
789 config_getSerialNumber(OUT char * sNumber);
790
800 int
801 config_getSerialNumber_Len(OUT char * sNumber, IN_OUT int * sNumberLen);
802
803
861 int
862 ctls_startTransaction(IN double amount, IN double amtOther, IN int type, IN const int _timeout, IN BYTE * tags,
863 IN int tagsLen);
864
865
920 int
921 ctls_activateTransaction(IN const int _timeout, IN BYTE * tags, IN int tagsLen);
922
923
934 int
935 ctls_cancelTransaction();
936
937
950 int
951 ctls_retrieveApplicationData(IN BYTE * AID, IN int AIDLen, OUT BYTE * tlv, IN_OUT int * tlvLen);
952
968 int
969 ctls_setApplicationData(IN BYTE * tlv, IN int tlvLen);
970
980 int
981 ctls_removeApplicationData(IN BYTE * AID, IN int AIDLen);
982
992 int
993 ctls_removeAllApplicationData();
994
1006 int
1007 ctls_retrieveAIDList(OUT BYTE * AIDList, IN_OUT int * AIDListLen);
1008
1022 int
1023 ctls_retrieveTerminalData(OUT BYTE * tlv, IN_OUT int * tlvLen);
1024
1039 int
1040 ctls_setTerminalData(IN BYTE * tlv, IN int tlvLen);
1041
1063 int
1064 ctls_retrieveCAPK(IN BYTE * capk, IN int capkLen, OUT BYTE * key, IN_OUT int * keyLen);
1065
1084 int
1085 ctls_setCAPK(IN BYTE * capk, IN int capkLen);
1086
1097 int
1098 ctls_removeCAPK(IN BYTE * capk, IN int capkLen);
1099
1108 int
1109 ctls_removeAllCAPK();
1110
1121 int
1122 ctls_retrieveCAPKList(OUT BYTE * keys, IN_OUT int * keysLen);
1123
1139 int
1140 ctls_setConfigurationGroup(IN BYTE * tlv, IN int tlvLen);
1141
1156 int
1157 ctls_getConfigurationGroup(IN int group, OUT BYTE * tlv, OUT int * tlvLen);
1158
1171 int
1172 ctls_getAllConfigurationGroups(OUT BYTE * tlv, IN_OUT int * tlvLen);
1173
1184 int
1185 ctls_removeConfigurationGroup(int group);
1186
1187
1192 void
1193 emv_allowFallback(IN int allow);
1194
1200 void
1201 emv_setAutoAuthenticateTransaction(IN int authenticate);
1202
1208 void
1209 emv_setAutoCompleteTransaction(IN int complete);
1210
1215 int
1216 emv_getAutoAuthenticateTransaction();
1217
1222 int
1223 emv_getAutoCompleteTransaction();
1224
1243 void
1244 emv_setTransactionParameters(IN double amount, IN double amtOther, IN int type, IN int timeout, IN BYTE * tags,
1245 IN int tagsLen);
1246
1268 int
1269 emv_startTransaction(IN double amount, IN double amtOther, IN int exponent, IN int type, IN int timeout, IN BYTE * tags,
1270 IN int tagsLen, IN int forceOnline);
1271
1272
1291 int
1292 emv_activateTransaction(IN int timeout, IN BYTE * tags, IN int tagsLen, IN int forceOnline);
1293
1310 int
1311 emv_authenticateTransaction(IN BYTE * updatedTLV, IN int updatedTLVLen);
1312
1330 int
1331 emv_authenticateTransactionWithTimeout(IN int timeout, IN BYTE * updatedTLV, IN int updatedTLVLen);
1332
1352 int
1353 emv_completeTransaction(IN int commError, IN BYTE * authCode, IN int authCodeLen,
1354 IN BYTE * iad, IN int iadLen, IN BYTE * tlvScripts, IN int tlvScriptsLen, IN BYTE * tlv, IN int tlvLen);
1355
1362 int
1363 emv_cancelTransaction();
1364
1377 int
1378 emv_retrieveApplicationData(IN BYTE * AID, IN int AIDLen, OUT BYTE * tlv, IN_OUT int * tlvLen);
1379
1392 int
1393 emv_setApplicationData(IN BYTE * name, IN int nameLen, IN BYTE * tlv, IN int tlvLen);
1394
1407 int
1408 emv_setApplicationDataTLV(IN BYTE * tlv, IN int tlvLen);
1409
1419 int
1420 emv_removeApplicationData(IN BYTE * AID, IN int AIDLen);
1421
1431 int
1432 emv_removeAllApplicationData();
1433
1445 int
1446 emv_retrieveAIDList(OUT BYTE * AIDList, IN_OUT int * AIDListLen);
1447
1461 int
1462 emv_retrieveTerminalData(OUT BYTE * tlv, IN_OUT int * tlvLen);
1463
1478 int
1479 emv_setTerminalData(IN BYTE * tlv, IN int tlvLen);
1480
1494 int
1495 emv_setTerminalMajorConfiguration(IN int configuration);
1496
1518 int
1519 emv_retrieveCAPK(IN BYTE * capk, IN int capkLen, OUT BYTE * key, IN_OUT int * keyLen);
1520
1539 int
1540 emv_setCAPK(IN BYTE * capk, IN int capkLen);
1541
1552 int
1553 emv_removeCAPK(IN BYTE * capk, IN int capkLen);
1554
1563 int
1564 emv_removeAllCAPK();
1565
1576 int
1577 emv_retrieveCAPKList(OUT BYTE * keys, IN_OUT int * keysLen);
1578
1589 int
1590 emv_retrieveCRL(OUT BYTE * list, IN_OUT int * lssLen);
1591
1604 int
1605 emv_setCRL(IN BYTE * list, IN int lsLen);
1606
1617 int
1618 emv_removeCRL(IN BYTE * list, IN int lsLen);
1619
1629 int
1630 emv_removeAllCRL();
1631
1642 int
1643 icc_getICCReaderStatus(OUT BYTE * status);
1644
1654 int
1655 icc_powerOnICC(OUT BYTE * ATR,
1656 IN_OUT int * inLen);
1657
1668 int
1669 icc_powerOffICC();
1670
1685 int
1686 icc_exchangeAPDU(IN BYTE * c_APDU,
1687 IN int cLen,
1688 OUT BYTE * reData,
1689 IN_OUT int * reLen);
1690
1696 int
1697 msr_cancelMSRSwipe();
1698
1707 int
1708 msr_startMSRSwipe(IN int _timeout);
1709
1723 int
1724 executeTransaction(WorldPayData * data, pWP_callBack wpCallback, int requestOnly);
1725
1730 int
1731 cancelWorldPay();
1732
1739 void
1740 parseMSRData(IN BYTE * resData, IN int resLen, IN_OUT IDTMSRData * cardData);
1741
1742 # ifdef __cplusplus
1743 }
1744 # endif
1745
1746
1747 #endif // ifndef __LIBIDT_VP3300_USB_H___
1748
pPIN_callBack
void(* pPIN_callBack)(int, IDTPINData *)
Definition: libIDT_VP3300_USB.h:51
device_getCurrentDeviceType
int device_getCurrentDeviceType()
emv_setAutoAuthenticateTransaction
void emv_setAutoAuthenticateTransaction(IN int authenticate)
ctls_getAllConfigurationGroups
int ctls_getAllConfigurationGroups(OUT BYTE *tlv, IN_OUT int *tlvLen)
device_setMerchantRecord
int device_setMerchantRecord(int index, int enabled, char *merchantID, char *merchantURL)
emv_getAutoCompleteTransaction
int emv_getAutoCompleteTransaction()
device_close
int device_close()
device_startTransaction
int device_startTransaction(IN double amount, IN double amtOther, IN int type, IN const int _timeout, IN BYTE *tags, IN int tagsLen)
emv_allowFallback
void emv_allowFallback(IN int allow)
emv_setTransactionParameters
void emv_setTransactionParameters(IN double amount, IN double amtOther, IN int type, IN int timeout, IN BYTE *tags, IN int tagsLen)
ctls_setConfigurationGroup
int ctls_setConfigurationGroup(IN BYTE *tlv, IN int tlvLen)
device_getTransactionResults
int device_getTransactionResults(IDTMSRData *cardData)
device_activateTransaction
int device_activateTransaction(IN const int _timeout, IN BYTE *tags, IN int tagsLen)
cancelWorldPay
int cancelWorldPay()
pSendDataLog
void(* pSendDataLog)(BYTE *, int)
Definition: libIDT_VP3300_USB.h:21
msr_cancelMSRSwipe
int msr_cancelMSRSwipe()
emv_startTransaction
int emv_startTransaction(IN double amount, IN double amtOther, IN int exponent, IN int type, IN int timeout, IN BYTE *tags, IN int tagsLen, IN int forceOnline)
emv_registerCallBk
void emv_registerCallBk(pEMV_callBack pEMVf)
ctls_cancelTransaction
int ctls_cancelTransaction()
ctls_retrieveCAPK
int ctls_retrieveCAPK(IN BYTE *capk, IN int capkLen, OUT BYTE *key, IN_OUT int *keyLen)
device_setThreadStackSize
void device_setThreadStackSize(int threadSize)
emv_retrieveCAPK
int emv_retrieveCAPK(IN BYTE *capk, IN int capkLen, OUT BYTE *key, IN_OUT int *keyLen)
pin_registerCallBk
void pin_registerCallBk(pPIN_callBack pPINf)
emv_activateTransaction
int emv_activateTransaction(IN int timeout, IN BYTE *tags, IN int tagsLen, IN int forceOnline)
device_registerCameraCallBk
void device_registerCameraCallBk(pCMR_callBack pCMRf)
ctls_getConfigurationGroup
int ctls_getConfigurationGroup(IN int group, OUT BYTE *tlv, OUT int *tlvLen)
icc_powerOnICC
int icc_powerOnICC(OUT BYTE *ATR, IN_OUT int *inLen)
emv_removeAllCRL
int emv_removeAllCRL()
emv_setApplicationDataTLV
int emv_setApplicationDataTLV(IN BYTE *tlv, IN int tlvLen)
OUT
#define OUT
device_setCurrentDevice
int device_setCurrentDevice(int deviceType)
emv_authenticateTransactionWithTimeout
int emv_authenticateTransactionWithTimeout(IN int timeout, IN BYTE *updatedTLV, IN int updatedTLVLen)
ctls_setCAPK
int ctls_setCAPK(IN BYTE *capk, IN int capkLen)
emv_setTerminalData
int emv_setTerminalData(IN BYTE *tlv, IN int tlvLen)
ctls_setTerminalData
int ctls_setTerminalData(IN BYTE *tlv, IN int tlvLen)
device_isConnected
int device_isConnected()
device_getMerchantRecord
int device_getMerchantRecord(IN int index, OUT BYTE *record)
device_setSDKWaitTime
void device_setSDKWaitTime(int waitTime)
device_getSDKWaitTime
int device_getSDKWaitTime()
emv_setAutoCompleteTransaction
void emv_setAutoCompleteTransaction(IN int complete)
pCSFS_callBack
void(* pCSFS_callBack)(BYTE status)
Definition: libIDT_VP3300_USB.h:63
emv_removeAllApplicationData
int emv_removeAllApplicationData()
emv_cancelTransaction
int emv_cancelTransaction()
ctls_setApplicationData
int ctls_setApplicationData(IN BYTE *tlv, IN int tlvLen)
msr_registerCallBk
void msr_registerCallBk(pMSR_callBack pMSRf)
IN
#define IN
device_getThreadStackSize
int device_getThreadStackSize()
device_setRTCDateTime
int device_setRTCDateTime(IN BYTE *dateTime, IN int dateTimeLen)
registerLogCallBk
void registerLogCallBk(pSendDataLog pFSend, pReadDataLog pFRead)
device_getFirmwareVersion_Len
int device_getFirmwareVersion_Len(OUT char *firmwareVersion, IN_OUT int *firmwareVersionLen)
SDK_Version
char * SDK_Version()
device_init
int device_init()
emv_removeCRL
int emv_removeCRL(IN BYTE *list, IN int lsLen)
ftpComm_callBack
void(* ftpComm_callBack)(int, int, int)
Definition: libIDT_VP3300_USB.h:83
device_setBurstMode
int device_setBurstMode(IN BYTE mode)
ctls_removeConfigurationGroup
int ctls_removeConfigurationGroup(int group)
executeTransaction
int executeTransaction(WorldPayData *data, pWP_callBack wpCallback, int requestOnly)
ctls_registerCallBk
void ctls_registerCallBk(pMSR_callBack pCTLSf)
emv_setTerminalMajorConfiguration
int emv_setTerminalMajorConfiguration(IN int configuration)
msr_startMSRSwipe
int msr_startMSRSwipe(IN int _timeout)
parseMSRData
void parseMSRData(IN BYTE *resData, IN int resLen, IN_OUT IDTMSRData *cardData)
emv_removeApplicationData
int emv_removeApplicationData(IN BYTE *AID, IN int AIDLen)
msr_registerCallBkp
void msr_registerCallBkp(pMSR_callBackp pMSRf)
device_registerRKICallBk
void device_registerRKICallBk(pRKI_callBack pRKIf)
ctls_removeAllCAPK
int ctls_removeAllCAPK()
emv_removeAllCAPK
int emv_removeAllCAPK()
emv_authenticateTransaction
int emv_authenticateTransaction(IN BYTE *updatedTLV, IN int updatedTLVLen)
comm_registerHTTPCallback
void comm_registerHTTPCallback(httpComm_callBack cBack)
device_getFirmwareVersion
int device_getFirmwareVersion(OUT char *firmwareVersion)
ctls_registerCallBkp
void ctls_registerCallBkp(pMSR_callBackp pCTLSf)
IN_OUT
#define IN_OUT
emv_setCAPK
int emv_setCAPK(IN BYTE *capk, IN int capkLen)
config_getSerialNumber_Len
int config_getSerialNumber_Len(OUT char *sNumber, IN_OUT int *sNumberLen)
setAbsoluteLibraryPath
int setAbsoluteLibraryPath(const char *absoluteLibraryPath)
device_isAttached
int device_isAttached(int deviceType)
pWP_callBack
void(* pWP_callBack)(char *, int, int)
Definition: libIDT_Device.h:53
emv_retrieveCAPKList
int emv_retrieveCAPKList(OUT BYTE *keys, IN_OUT int *keysLen)
emv_retrieveTerminalData
int emv_retrieveTerminalData(OUT BYTE *tlv, IN_OUT int *tlvLen)
emv_removeCAPK
int emv_removeCAPK(IN BYTE *capk, IN int capkLen)
device_cancelTransaction
int device_cancelTransaction()
v4Comm_callBack
void(* v4Comm_callBack)(BYTE, BYTE, BYTE *, int)
Definition: libIDT_VP3300_USB.h:97
icc_getICCReaderStatus
int icc_getICCReaderStatus(OUT BYTE *status)
device_registerCardStatusFrontSwitchCallBk
void device_registerCardStatusFrontSwitchCallBk(pCSFS_callBack pCSFSf)
emv_retrieveApplicationData
int emv_retrieveApplicationData(IN BYTE *AID, IN int AIDLen, OUT BYTE *tlv, IN_OUT int *tlvLen)
ctls_retrieveCAPKList
int ctls_retrieveCAPKList(OUT BYTE *keys, IN_OUT int *keysLen)
emv_retrieveAIDList
int emv_retrieveAIDList(OUT BYTE *AIDList, IN_OUT int *AIDListLen)
emv_completeTransaction
int emv_completeTransaction(IN int commError, IN BYTE *authCode, IN int authCodeLen, IN BYTE *iad, IN int iadLen, IN BYTE *tlvScripts, IN int tlvScriptsLen, IN BYTE *tlv, IN int tlvLen)
emv_setApplicationData
int emv_setApplicationData(IN BYTE *name, IN int nameLen, IN BYTE *tlv, IN int tlvLen)
device_enablePassThrough
int device_enablePassThrough(int enablePassThrough)
ctls_removeAllApplicationData
int ctls_removeAllApplicationData()
ctls_removeApplicationData
int ctls_removeApplicationData(IN BYTE *AID, IN int AIDLen)
emv_getAutoAuthenticateTransaction
int emv_getAutoAuthenticateTransaction()
device_getRTCDateTime
int device_getRTCDateTime(IN BYTE *dateTime, IN_OUT int *dateTimeLen)
pMSR_callBack
void(* pMSR_callBack)(int, IDTMSRData)
Definition: libIDT_VP3300_USB.h:39
pEMV_callBack
void(* pEMV_callBack)(int, int, BYTE *, int, IDTTransactionData *, EMV_Callback *, int)
Definition: libIDT_VP3300_USB.h:33
registerHotplugCallBk
void registerHotplugCallBk(pMessageHotplug pMsgHotplug)
device_setTransactionExponent
void device_setTransactionExponent(int exponent)
pReadDataLog
void(* pReadDataLog)(BYTE *, int)
Definition: libIDT_VP3300_USB.h:27
device_startRKI
int device_startRKI(const char *caPath, int isProduction)
emv_retrieveCRL
int emv_retrieveCRL(OUT BYTE *list, IN_OUT int *lssLen)
ctls_startTransaction
int ctls_startTransaction(IN double amount, IN double amtOther, IN int type, IN const int _timeout, IN BYTE *tags, IN int tagsLen)
pMessageHotplug
void(* pMessageHotplug)(int, int)
Definition: libIDT_VP3300_USB.h:15
device_SendDataCommandNEO
int device_SendDataCommandNEO(IN int cmd, IN int subCmd, IN BYTE *data, IN int dataLen, OUT BYTE *response, IN_OUT int *respLen)
httpComm_callBack
void(* httpComm_callBack)(BYTE *, int)
Definition: libIDT_VP3300_USB.h:89
config_getSerialNumber
int config_getSerialNumber(OUT char *sNumber)
pCMR_callBack
void(* pCMR_callBack)(int, IDTCMRData *)
Definition: libIDT_VP3300_USB.h:57
ctls_retrieveAIDList
int ctls_retrieveAIDList(OUT BYTE *AIDList, IN_OUT int *AIDListLen)
device_setPollMode
int device_setPollMode(IN BYTE mode)
device_pingDevice
int device_pingDevice()
pMSR_callBackp
void(* pMSR_callBackp)(int, IDTMSRData *)
Definition: libIDT_VP3300_USB.h:45
ctls_retrieveApplicationData
int ctls_retrieveApplicationData(IN BYTE *AID, IN int AIDLen, OUT BYTE *tlv, IN_OUT int *tlvLen)
device_getIDGStatusCodeString
void device_getIDGStatusCodeString(IN int returnCode, OUT char *despcrition)
pRKI_callBack
void(* pRKI_callBack)(int, char *)
Definition: libIDT_VP3300_USB.h:69
device_controlUserInterface
int device_controlUserInterface(IN BYTE *values)
ctls_retrieveTerminalData
int ctls_retrieveTerminalData(OUT BYTE *tlv, IN_OUT int *tlvLen)
comm_registerV4Callback
void comm_registerV4Callback(v4Comm_callBack cBack)
emv_setCRL
int emv_setCRL(IN BYTE *list, IN int lsLen)
icc_powerOffICC
int icc_powerOffICC()
ctls_removeCAPK
int ctls_removeCAPK(IN BYTE *capk, IN int capkLen)
icc_exchangeAPDU
int icc_exchangeAPDU(IN BYTE *c_APDU, IN int cLen, OUT BYTE *reData, IN_OUT int *reLen)
device_getMerchantRecord_Len
int device_getMerchantRecord_Len(IN int index, OUT BYTE *record, IN_OUT int *recordLen)
ctls_activateTransaction
int ctls_activateTransaction(IN const int _timeout, IN BYTE *tags, IN int tagsLen)