| IDTech Universal SDK 1.0.35.027 API reference for C++

libIDT_VP3300_BT.h
Go to the documentation of this file.
1 #ifndef __LIBIDT_VP3300_BT_H___
2 # define __LIBIDT_VP3300_BT_H___
3
4
5 # define IN
6 # define OUT
7 # define IN_OUT
8 # include "IDTDef.h"
9
15 typedef void (* pMessageHotplug)(int, int);
16
21 typedef void (* pSendDataLog)(BYTE *, int);
22
27 typedef void (* pReadDataLog)(BYTE *, int);
28
33 typedef void (* pEMV_callBack)(int, int, BYTE *, int, IDTTransactionData *, EMV_Callback *, int);
34
39 typedef void (* pMSR_callBack)(int, IDTMSRData);
40
45 typedef void (* pMSR_callBackp)(int, IDTMSRData *);
46
51 typedef void (* pPIN_callBack)(int, IDTPINData *);
52
57 typedef void (* pCMR_callBack)(int, IDTCMRData *);
58
63 typedef void (* pCSFS_callBack)(BYTE status);
64
69 typedef void (* pRKI_callBack)(int,
70 char *);
71
83 typedef void (* ftpComm_callBack)(int, int, int);
84
89 typedef void (* httpComm_callBack)(BYTE *, int);
90
97 typedef void (* v4Comm_callBack)(BYTE, BYTE, BYTE *, int);
98
99
100 # ifdef __cplusplus
101 extern "C" {
102 # endif
103
107 void
108 registerHotplugCallBk(pMessageHotplug pMsgHotplug);
109
113 void
114 registerLogCallBk(pSendDataLog pFSend, pReadDataLog pFRead);
115
120 void
121 device_registerRKICallBk(pRKI_callBack pRKIf);
122
126 void
127 emv_registerCallBk(pEMV_callBack pEMVf);
128
132 void
133 msr_registerCallBk(pMSR_callBack pMSRf);
134
138 void
139 msr_registerCallBkp(pMSR_callBackp pMSRf);
140
144 void
145 ctls_registerCallBk(pMSR_callBack pCTLSf);
146
150 void
151 ctls_registerCallBkp(pMSR_callBackp pCTLSf);
152
156 void
157 pin_registerCallBk(pPIN_callBack pPINf);
158
162 void
163 device_registerCameraCallBk(pCMR_callBack pCMRf);
164
168 void
169 device_registerCardStatusFrontSwitchCallBk(pCSFS_callBack pCSFSf);
170
176 void
177 comm_registerHTTPCallback(httpComm_callBack cBack);
178
184 void
185 comm_registerV4Callback(v4Comm_callBack cBack);
186
191 char *
192 SDK_Version();
193
202 int
203 setAbsoluteLibraryPath(const char * absoluteLibraryPath);
204
212 int
213 device_init();
214
256 int
257 device_setCurrentDevice(int deviceType);
258
264 int
265 device_close();
266
267
327 void
328 device_getIDGStatusCodeString(IN int returnCode, OUT char * despcrition);
329
330
335 int
336 device_isConnected();
337
344 int
345 device_isAttached(int deviceType);
346
357 int
358 device_getFirmwareVersion(OUT char * firmwareVersion);
359
369 int
370 device_getFirmwareVersion_Len(OUT char * firmwareVersion, IN_OUT int * firmwareVersionLen);
371
380 int
381 device_pingDevice();
382
425 int
426 device_controlUserInterface(IN BYTE * values);
427
433 int
434 device_getCurrentDeviceType();
435
436
438 // * Send a Command to device
439 // *
440 // * Sends a command to the device .
441 // *
442 // * @param cmd buffer of command to execute.
443 // * @param cmdLen, the length of the buffer cmd.
444 // *
445 // * @param data buffer of IDG command data.
446 // * @param dataLen, the length of the buffer data.
447 // *
448 // * @param response Response data
449 // * @param respLen, the length of Response data
450 //
451 // * @return RETURN_CODE: Values can be parsed with device_getIDGStatusCodeString()
452 // */
453 //
454 // int device_SendDataCommand(IN BYTE* cmd, IN int cmdLen, IN BYTE* data, IN int dataLen, OUT BYTE* response, IN_OUT int *respLen);
455
472 int
473 device_SendDataCommandNEO(IN int cmd, IN int subCmd, IN BYTE * data, IN int dataLen, OUT BYTE * response,
474 IN_OUT int * respLen);
475
486 int
487 device_enablePassThrough(int enablePassThrough);
488
499 int
500 device_setBurstMode(IN BYTE mode);
501
511 int
512 device_setPollMode(IN BYTE mode);
513
526 int
527 device_setMerchantRecord(int index, int enabled, char * merchantID, char * merchantURL);
528
550 int
551 device_getMerchantRecord(IN int index,
552 OUT BYTE * record);
553
574 int
575 device_getMerchantRecord_Len(IN int index,
576 OUT BYTE * record, IN_OUT int * recordLen);
577
587 int
588 device_getTransactionResults(IDTMSRData * cardData);
589
647 int
648 device_startTransaction(IN double amount, IN double amtOther, IN int type, IN const int _timeout, IN BYTE * tags,
649 IN int tagsLen);
650
655 void
656 device_setTransactionExponent(int exponent);
657
712 int
713 device_activateTransaction(IN const int _timeout, IN BYTE * tags, IN int tagsLen);
714
720 int
721 device_cancelTransaction();
722
737 int
738 device_getRTCDateTime(IN BYTE * dateTime, IN_OUT int * dateTimeLen);
739
753 int
754 device_setRTCDateTime(IN BYTE * dateTime, IN int dateTimeLen);
755
765 int
766 device_startRKI(const char * caPath, int isProduction);
767
776 int
777 device_getSDKWaitTime();
778
788 void
789 device_setSDKWaitTime(int waitTime);
790
799 int
800 device_getThreadStackSize();
801
809 void
810 device_setThreadStackSize(int threadSize);
811
822 int
823 config_getSerialNumber(OUT char * sNumber);
824
834 int
835 config_getSerialNumber_Len(OUT char * sNumber, IN_OUT int * sNumberLen);
836
894 int
895 ctls_startTransaction(IN double amount, IN double amtOther, IN int type, IN const int _timeout, IN BYTE * tags,
896 IN int tagsLen);
897
898
953 int
954 ctls_activateTransaction(IN const int _timeout, IN BYTE * tags, IN int tagsLen);
955
956
967 int
968 ctls_cancelTransaction();
969
970
983 int
984 ctls_retrieveApplicationData(IN BYTE * AID, IN int AIDLen, OUT BYTE * tlv, IN_OUT int * tlvLen);
985
1001 int
1002 ctls_setApplicationData(IN BYTE * tlv, IN int tlvLen);
1003
1013 int
1014 ctls_removeApplicationData(IN BYTE * AID, IN int AIDLen);
1015
1025 int
1026 ctls_removeAllApplicationData();
1027
1039 int
1040 ctls_retrieveAIDList(OUT BYTE * AIDList, IN_OUT int * AIDListLen);
1041
1055 int
1056 ctls_retrieveTerminalData(OUT BYTE * tlv, IN_OUT int * tlvLen);
1057
1072 int
1073 ctls_setTerminalData(IN BYTE * tlv, IN int tlvLen);
1074
1096 int
1097 ctls_retrieveCAPK(IN BYTE * capk, IN int capkLen, OUT BYTE * key, IN_OUT int * keyLen);
1098
1117 int
1118 ctls_setCAPK(IN BYTE * capk, IN int capkLen);
1119
1130 int
1131 ctls_removeCAPK(IN BYTE * capk, IN int capkLen);
1132
1141 int
1142 ctls_removeAllCAPK();
1143
1154 int
1155 ctls_retrieveCAPKList(OUT BYTE * keys, IN_OUT int * keysLen);
1156
1172 int
1173 ctls_setConfigurationGroup(IN BYTE * tlv, IN int tlvLen);
1174
1189 int
1190 ctls_getConfigurationGroup(IN int group, OUT BYTE * tlv, OUT int * tlvLen);
1191
1204 int
1205 ctls_getAllConfigurationGroups(OUT BYTE * tlv, IN_OUT int * tlvLen);
1206
1217 int
1218 ctls_removeConfigurationGroup(int group);
1219
1220
1225 void
1226 emv_allowFallback(IN int allow);
1227
1233 void
1234 emv_setAutoAuthenticateTransaction(IN int authenticate);
1235
1241 void
1242 emv_setAutoCompleteTransaction(IN int complete);
1243
1248 int
1249 emv_getAutoAuthenticateTransaction();
1250
1255 int
1256 emv_getAutoCompleteTransaction();
1257
1276 void
1277 emv_setTransactionParameters(IN double amount, IN double amtOther, IN int type, IN int timeout, IN BYTE * tags,
1278 IN int tagsLen);
1279
1301 int
1302 emv_startTransaction(IN double amount, IN double amtOther, IN int exponent, IN int type, IN int timeout, IN BYTE * tags,
1303 IN int tagsLen, IN int forceOnline);
1304
1305
1324 int
1325 emv_activateTransaction(IN int timeout, IN BYTE * tags, IN int tagsLen, IN int forceOnline);
1326
1343 int
1344 emv_authenticateTransaction(IN BYTE * updatedTLV, IN int updatedTLVLen);
1345
1363 int
1364 emv_authenticateTransactionWithTimeout(IN int timeout, IN BYTE * updatedTLV, IN int updatedTLVLen);
1365
1385 int
1386 emv_completeTransaction(IN int commError, IN BYTE * authCode, IN int authCodeLen,
1387 IN BYTE * iad, IN int iadLen, IN BYTE * tlvScripts, IN int tlvScriptsLen, IN BYTE * tlv, IN int tlvLen);
1388
1395 int
1396 emv_cancelTransaction();
1397
1410 int
1411 emv_retrieveApplicationData(IN BYTE * AID, IN int AIDLen, OUT BYTE * tlv, IN_OUT int * tlvLen);
1412
1425 int
1426 emv_setApplicationData(IN BYTE * name, IN int nameLen, IN BYTE * tlv, IN int tlvLen);
1427
1440 int
1441 emv_setApplicationDataTLV(IN BYTE * tlv, IN int tlvLen);
1442
1452 int
1453 emv_removeApplicationData(IN BYTE * AID, IN int AIDLen);
1454
1464 int
1465 emv_removeAllApplicationData();
1466
1478 int
1479 emv_retrieveAIDList(OUT BYTE * AIDList, IN_OUT int * AIDListLen);
1480
1494 int
1495 emv_retrieveTerminalData(OUT BYTE * tlv, IN_OUT int * tlvLen);
1496
1511 int
1512 emv_setTerminalData(IN BYTE * tlv, IN int tlvLen);
1513
1527 int
1528 emv_setTerminalMajorConfiguration(IN int configuration);
1529
1551 int
1552 emv_retrieveCAPK(IN BYTE * capk, IN int capkLen, OUT BYTE * key, IN_OUT int * keyLen);
1553
1572 int
1573 emv_setCAPK(IN BYTE * capk, IN int capkLen);
1574
1585 int
1586 emv_removeCAPK(IN BYTE * capk, IN int capkLen);
1587
1596 int
1597 emv_removeAllCAPK();
1598
1609 int
1610 emv_retrieveCAPKList(OUT BYTE * keys, IN_OUT int * keysLen);
1611
1622 int
1623 emv_retrieveCRL(OUT BYTE * list, IN_OUT int * lssLen);
1624
1637 int
1638 emv_setCRL(IN BYTE * list, IN int lsLen);
1639
1650 int
1651 emv_removeCRL(IN BYTE * list, IN int lsLen);
1652
1662 int
1663 emv_removeAllCRL();
1664
1675 int
1676 icc_getICCReaderStatus(OUT BYTE * status);
1677
1687 int
1688 icc_powerOnICC(OUT BYTE * ATR,
1689 IN_OUT int * inLen);
1690
1701 int
1702 icc_powerOffICC();
1703
1718 int
1719 icc_exchangeAPDU(IN BYTE * c_APDU,
1720 IN int cLen,
1721 OUT BYTE * reData,
1722 IN_OUT int * reLen);
1723
1729 int
1730 msr_cancelMSRSwipe();
1731
1739 int
1740 msr_startMSRSwipe(IN int _timeout);
1741
1742
1743 int
1744 msr_startMSRSwipe(IN int _timeout);
1745
1746
1760 int
1761 executeTransaction(WorldPayData * data, pWP_callBack wpCallback, int requestOnly);
1762
1767 int
1768 cancelWorldPay();
1769
1776 void
1777 parseMSRData(IN BYTE * resData, IN int resLen, IN_OUT IDTMSRData * cardData);
1778
1779 # ifdef __cplusplus
1780 }
1781 # endif
1782
1783
1784 #endif // ifndef __LIBIDT_VP3300_BT_H___
1785
emv_startTransaction
int emv_startTransaction(IN double amount, IN double amtOther, IN int exponent, IN int type, IN int timeout, IN BYTE *tags, IN int tagsLen, IN int forceOnline)
ctls_registerCallBk
void ctls_registerCallBk(pMSR_callBack pCTLSf)
device_close
int device_close()
httpComm_callBack
void(* httpComm_callBack)(BYTE *, int)
Definition: libIDT_VP3300_BT.h:89
emv_removeApplicationData
int emv_removeApplicationData(IN BYTE *AID, IN int AIDLen)
ctls_startTransaction
int ctls_startTransaction(IN double amount, IN double amtOther, IN int type, IN const int _timeout, IN BYTE *tags, IN int tagsLen)
emv_retrieveAIDList
int emv_retrieveAIDList(OUT BYTE *AIDList, IN_OUT int *AIDListLen)
ctls_setApplicationData
int ctls_setApplicationData(IN BYTE *tlv, IN int tlvLen)
ctls_setCAPK
int ctls_setCAPK(IN BYTE *capk, IN int capkLen)
IN_OUT
#define IN_OUT
ctls_setTerminalData
int ctls_setTerminalData(IN BYTE *tlv, IN int tlvLen)
device_setTransactionExponent
void device_setTransactionExponent(int exponent)
device_setThreadStackSize
void device_setThreadStackSize(int threadSize)
emv_cancelTransaction
int emv_cancelTransaction()
device_getCurrentDeviceType
int device_getCurrentDeviceType()
emv_allowFallback
void emv_allowFallback(IN int allow)
msr_startMSRSwipe
int msr_startMSRSwipe(IN int _timeout)
emv_removeAllApplicationData
int emv_removeAllApplicationData()
emv_retrieveCAPKList
int emv_retrieveCAPKList(OUT BYTE *keys, IN_OUT int *keysLen)
ctls_removeAllCAPK
int ctls_removeAllCAPK()
ctls_getConfigurationGroup
int ctls_getConfigurationGroup(IN int group, OUT BYTE *tlv, OUT int *tlvLen)
device_startRKI
int device_startRKI(const char *caPath, int isProduction)
pMSR_callBackp
void(* pMSR_callBackp)(int, IDTMSRData *)
Definition: libIDT_VP3300_BT.h:45
SDK_Version
char * SDK_Version()
device_registerCardStatusFrontSwitchCallBk
void device_registerCardStatusFrontSwitchCallBk(pCSFS_callBack pCSFSf)
pReadDataLog
void(* pReadDataLog)(BYTE *, int)
Definition: libIDT_VP3300_BT.h:27
device_registerRKICallBk
void device_registerRKICallBk(pRKI_callBack pRKIf)
comm_registerV4Callback
void comm_registerV4Callback(v4Comm_callBack cBack)
msr_cancelMSRSwipe
int msr_cancelMSRSwipe()
icc_powerOnICC
int icc_powerOnICC(OUT BYTE *ATR, IN_OUT int *inLen)
emv_setAutoAuthenticateTransaction
void emv_setAutoAuthenticateTransaction(IN int authenticate)
device_init
int device_init()
device_startTransaction
int device_startTransaction(IN double amount, IN double amtOther, IN int type, IN const int _timeout, IN BYTE *tags, IN int tagsLen)
ftpComm_callBack
void(* ftpComm_callBack)(int, int, int)
Definition: libIDT_VP3300_BT.h:83
executeTransaction
int executeTransaction(WorldPayData *data, pWP_callBack wpCallback, int requestOnly)
ctls_setConfigurationGroup
int ctls_setConfigurationGroup(IN BYTE *tlv, IN int tlvLen)
pPIN_callBack
void(* pPIN_callBack)(int, IDTPINData *)
Definition: libIDT_VP3300_BT.h:51
ctls_removeAllApplicationData
int ctls_removeAllApplicationData()
pMessageHotplug
void(* pMessageHotplug)(int, int)
Definition: libIDT_VP3300_BT.h:15
emv_authenticateTransactionWithTimeout
int emv_authenticateTransactionWithTimeout(IN int timeout, IN BYTE *updatedTLV, IN int updatedTLVLen)
device_setRTCDateTime
int device_setRTCDateTime(IN BYTE *dateTime, IN int dateTimeLen)
emv_setAutoCompleteTransaction
void emv_setAutoCompleteTransaction(IN int complete)
ctls_retrieveApplicationData
int ctls_retrieveApplicationData(IN BYTE *AID, IN int AIDLen, OUT BYTE *tlv, IN_OUT int *tlvLen)
registerHotplugCallBk
void registerHotplugCallBk(pMessageHotplug pMsgHotplug)
config_getSerialNumber_Len
int config_getSerialNumber_Len(OUT char *sNumber, IN_OUT int *sNumberLen)
ctls_removeConfigurationGroup
int ctls_removeConfigurationGroup(int group)
device_setPollMode
int device_setPollMode(IN BYTE mode)
pSendDataLog
void(* pSendDataLog)(BYTE *, int)
Definition: libIDT_VP3300_BT.h:21
icc_exchangeAPDU
int icc_exchangeAPDU(IN BYTE *c_APDU, IN int cLen, OUT BYTE *reData, IN_OUT int *reLen)
ctls_registerCallBkp
void ctls_registerCallBkp(pMSR_callBackp pCTLSf)
emv_getAutoCompleteTransaction
int emv_getAutoCompleteTransaction()
OUT
#define OUT
ctls_removeApplicationData
int ctls_removeApplicationData(IN BYTE *AID, IN int AIDLen)
pin_registerCallBk
void pin_registerCallBk(pPIN_callBack pPINf)
device_getRTCDateTime
int device_getRTCDateTime(IN BYTE *dateTime, IN_OUT int *dateTimeLen)
pEMV_callBack
void(* pEMV_callBack)(int, int, BYTE *, int, IDTTransactionData *, EMV_Callback *, int)
Definition: libIDT_VP3300_BT.h:33
setAbsoluteLibraryPath
int setAbsoluteLibraryPath(const char *absoluteLibraryPath)
device_getFirmwareVersion_Len
int device_getFirmwareVersion_Len(OUT char *firmwareVersion, IN_OUT int *firmwareVersionLen)
emv_retrieveApplicationData
int emv_retrieveApplicationData(IN BYTE *AID, IN int AIDLen, OUT BYTE *tlv, IN_OUT int *tlvLen)
device_getFirmwareVersion
int device_getFirmwareVersion(OUT char *firmwareVersion)
ctls_cancelTransaction
int ctls_cancelTransaction()
device_setSDKWaitTime
void device_setSDKWaitTime(int waitTime)
cancelWorldPay
int cancelWorldPay()
emv_setCAPK
int emv_setCAPK(IN BYTE *capk, IN int capkLen)
device_registerCameraCallBk
void device_registerCameraCallBk(pCMR_callBack pCMRf)
emv_setApplicationData
int emv_setApplicationData(IN BYTE *name, IN int nameLen, IN BYTE *tlv, IN int tlvLen)
device_getThreadStackSize
int device_getThreadStackSize()
emv_setApplicationDataTLV
int emv_setApplicationDataTLV(IN BYTE *tlv, IN int tlvLen)
ctls_retrieveCAPKList
int ctls_retrieveCAPKList(OUT BYTE *keys, IN_OUT int *keysLen)
device_getIDGStatusCodeString
void device_getIDGStatusCodeString(IN int returnCode, OUT char *despcrition)
v4Comm_callBack
void(* v4Comm_callBack)(BYTE, BYTE, BYTE *, int)
Definition: libIDT_VP3300_BT.h:97
device_getSDKWaitTime
int device_getSDKWaitTime()
parseMSRData
void parseMSRData(IN BYTE *resData, IN int resLen, IN_OUT IDTMSRData *cardData)
emv_authenticateTransaction
int emv_authenticateTransaction(IN BYTE *updatedTLV, IN int updatedTLVLen)
ctls_removeCAPK
int ctls_removeCAPK(IN BYTE *capk, IN int capkLen)
pRKI_callBack
void(* pRKI_callBack)(int, char *)
Definition: libIDT_VP3300_BT.h:69
registerLogCallBk
void registerLogCallBk(pSendDataLog pFSend, pReadDataLog pFRead)
pWP_callBack
void(* pWP_callBack)(char *, int, int)
Definition: libIDT_Device.h:53
device_getTransactionResults
int device_getTransactionResults(IDTMSRData *cardData)
emv_getAutoAuthenticateTransaction
int emv_getAutoAuthenticateTransaction()
emv_retrieveTerminalData
int emv_retrieveTerminalData(OUT BYTE *tlv, IN_OUT int *tlvLen)
ctls_retrieveAIDList
int ctls_retrieveAIDList(OUT BYTE *AIDList, IN_OUT int *AIDListLen)
emv_removeCRL
int emv_removeCRL(IN BYTE *list, IN int lsLen)
emv_removeAllCAPK
int emv_removeAllCAPK()
ctls_activateTransaction
int ctls_activateTransaction(IN const int _timeout, IN BYTE *tags, IN int tagsLen)
ctls_getAllConfigurationGroups
int ctls_getAllConfigurationGroups(OUT BYTE *tlv, IN_OUT int *tlvLen)
config_getSerialNumber
int config_getSerialNumber(OUT char *sNumber)
msr_registerCallBk
void msr_registerCallBk(pMSR_callBack pMSRf)
emv_setTerminalMajorConfiguration
int emv_setTerminalMajorConfiguration(IN int configuration)
device_controlUserInterface
int device_controlUserInterface(IN BYTE *values)
emv_activateTransaction
int emv_activateTransaction(IN int timeout, IN BYTE *tags, IN int tagsLen, IN int forceOnline)
icc_getICCReaderStatus
int icc_getICCReaderStatus(OUT BYTE *status)
emv_setTransactionParameters
void emv_setTransactionParameters(IN double amount, IN double amtOther, IN int type, IN int timeout, IN BYTE *tags, IN int tagsLen)
emv_setTerminalData
int emv_setTerminalData(IN BYTE *tlv, IN int tlvLen)
comm_registerHTTPCallback
void comm_registerHTTPCallback(httpComm_callBack cBack)
device_getMerchantRecord_Len
int device_getMerchantRecord_Len(IN int index, OUT BYTE *record, IN_OUT int *recordLen)
IN
#define IN
ctls_retrieveCAPK
int ctls_retrieveCAPK(IN BYTE *capk, IN int capkLen, OUT BYTE *key, IN_OUT int *keyLen)
pCSFS_callBack
void(* pCSFS_callBack)(BYTE status)
Definition: libIDT_VP3300_BT.h:63
icc_powerOffICC
int icc_powerOffICC()
pCMR_callBack
void(* pCMR_callBack)(int, IDTCMRData *)
Definition: libIDT_VP3300_BT.h:57
emv_retrieveCAPK
int emv_retrieveCAPK(IN BYTE *capk, IN int capkLen, OUT BYTE *key, IN_OUT int *keyLen)
device_setCurrentDevice
int device_setCurrentDevice(int deviceType)
emv_removeCAPK
int emv_removeCAPK(IN BYTE *capk, IN int capkLen)
device_setMerchantRecord
int device_setMerchantRecord(int index, int enabled, char *merchantID, char *merchantURL)
device_pingDevice
int device_pingDevice()
device_activateTransaction
int device_activateTransaction(IN const int _timeout, IN BYTE *tags, IN int tagsLen)
device_isConnected
int device_isConnected()
device_isAttached
int device_isAttached(int deviceType)
ctls_retrieveTerminalData
int ctls_retrieveTerminalData(OUT BYTE *tlv, IN_OUT int *tlvLen)
emv_retrieveCRL
int emv_retrieveCRL(OUT BYTE *list, IN_OUT int *lssLen)
emv_registerCallBk
void emv_registerCallBk(pEMV_callBack pEMVf)
device_setBurstMode
int device_setBurstMode(IN BYTE mode)
device_enablePassThrough
int device_enablePassThrough(int enablePassThrough)
emv_completeTransaction
int emv_completeTransaction(IN int commError, IN BYTE *authCode, IN int authCodeLen, IN BYTE *iad, IN int iadLen, IN BYTE *tlvScripts, IN int tlvScriptsLen, IN BYTE *tlv, IN int tlvLen)
msr_registerCallBkp
void msr_registerCallBkp(pMSR_callBackp pMSRf)
device_cancelTransaction
int device_cancelTransaction()
emv_setCRL
int emv_setCRL(IN BYTE *list, IN int lsLen)
device_getMerchantRecord
int device_getMerchantRecord(IN int index, OUT BYTE *record)
pMSR_callBack
void(* pMSR_callBack)(int, IDTMSRData)
Definition: libIDT_VP3300_BT.h:39
emv_removeAllCRL
int emv_removeAllCRL()
device_SendDataCommandNEO
int device_SendDataCommandNEO(IN int cmd, IN int subCmd, IN BYTE *data, IN int dataLen, OUT BYTE *response, IN_OUT int *respLen)