| CustomiOSApi 1.06

- Main Page
- Classes

All Classes Functions Enumerations Enumerator Pages
CustomiOSApi Documentation

Document Overview
This document details about CUSTOM iOS API for printers. And also explains how to use this API for iOS application development for CUSTOM printers.

About CUSTOM iOS API
This API provides functions to access the CUSTOM printers via Bluetooth and Wifi. It includes below functions to access the printer

- Get the printer class for printer
- Connect to printer
- Close connection
- Set timeout for read/write
- Write / Read bytes to/from printer
- Print text with various text attributes
- Print image with image scaling options
- Print Barcode and Barcode 2D
- Cut, eject / retract and present the ticket

Printers Supported
This is the list of the printers type supported by this API:

- MY3
- MYPRINTER
- K3
- KPM216H ETH 200 dpi
- KPM216H ETH 300 dpi
- KPM302H
- KUBE
- KUBE ETHERNET
- Q1
- Q3
- VKP80II
- VKP80II ETHERNET
- TG2460H
- TG2480H
- D-ONE
- KPM150H
- KPM180H/TK180
- K80
- VK80
- VKP80III
- MYPRINTER
- KPM216H 200 dpi
- KPM216H 300 dpi
- TL60
- TL80
- TG02H
- PLUS2
- mPLUS2
- PLUS4
- TPTCM60III
- TPTCM112III